-------------------------------------------------------------------------------
-----------H----H--X----X-----CCCCC-----22222----0000-----0000-----11----------
----------H----H----X-X-----C--------------2---0----0---0----0---1-1-----------
---------HHHHHH-----X------C----------22222---0----0---0----0-----1------------
--------H----H----X--X----C----------2-------0----0---0----0-----1-------------
-------H----H---X-----X---CCCCC-----22222----0000-----0000----11111------------
-------------------------------------------------------------------------------
-- Contact: hxc2001<at>hxc2001.com ---------------------- http://hxc2001.com --
-------------------------------------------------------------------------------
HxC Floppy Emulator project
(c) 2006-2017 Jean-François DEL NERO / (c) HxC2001
-------------------------------------------------------------------------------

All the UPD firmware update files in this archive are usable when your drive have
the HxC Bootloader.

You can purchase the bootloader on this page : http://hxc2001.com/store/

USB STM32 HxC Floppy Emulator Update procedure :

	-> Copy the new firmware file (*.upd) to a FAT32/FAT16/FAT12 USB flash device.
	-> Insert the USB Stick into the emulator and press both buttons.
	-> Power up the device and keep the button pressed during at least 2 seconds.
	-> Wait some seconds... its done !

Note 1:
Bootstrap error codes:
	Error 1 : (blink 1 time and 2 seconds pause cycle)  No entry point (->no software flashed)
	Error 2 : (blink 2 time and 2 seconds pause cycle)  USB init error.
	Error 3 : (blink 3 time and 2 seconds pause cycle)  FAT error.
	Error 4 : (blink 4 time and 2 seconds pause cycle)  UPD File not found!
	Error 5 : (blink 5 time and 2 seconds pause cycle)  Bad UPD File header! (Bad UPD file)
	Error 6 : (blink 6 time and 2 seconds pause cycle)  Bad data crc! (UPD file corrupted)
	Error 7 : (blink 7 time and 2 seconds pause cycle)  Bad data size! (UPD file corrupted)
	Error 8 : (blink 8 time and 2 seconds pause cycle)  Write error (STM32 flash error)

Jeff / HxC2001
